FusWorth
AC12 Metal
Product Specifications
	Specification
	Details

	Dimensions
	107*74*19mm

	Standard
	Complies with ISO/IEC 14443 Type A

	Housing Material
	Metal

	Operating Voltage
	9-12VDC

	Operating Current
	70mA

	Supported Card
	MIFARE One IC card

	Keypad
	Touch keypad with LED digits

	Operating Frequency
	IC (13.56MHz)

	Operating Environment
	Operating Temperature: -10~50℃ Operating Humidity: <90%< p="">

	Transmission Distance
	80m max.

	Reading Distance
	IC 3-5cm depending on card

	Output Mode
	WG26/34

	Pulse Output
	Negative pulse widthTP=100μs, Pulse periodTW=2ms






