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Product Specifications
	Specification
	Details

	Source Specification
	Metal Card Reader

	Main Unit Dimensions
	88*88*18mm

	Back Cover Dimensions
	86*86*2mm

	Standard
	Complies with ISO/IEC 14443 Type A

	Housing Material
	Metal

	Operating Voltage
	9-12VDC

	Operating Current
	70mA

	Protection Rating
	Waterproof and Dustproof (IP65)

	Supported Card
	MIFARE One IC card

	Keypad
	Touch keypad with LED digits

	Operating Frequency
	IC (13.56MHz)

	Operating Environment
	Operating Temperature: -10~50℃ Operating Humidity: <90%< p="">

	Transmission Distance
	80m max.

	Reading Distance
	IC 3-5cm depending on card

	Output Mode
	WG26/34

	Pulse Output
	Negative pulse widthTP=100μs, Pulse periodTW=2ms






