FusWorth
AC15-E
Product Specifications
	Specification
	Details

	Source Specification
	Anti-Copy Metal Card Reader

	Dimensions
	88*88*18mm

	Source Specification
	Standard Complies with ISO/IEC 14443 Type A

	Source Specification
	Operating Voltage 9-12VDC

	Source Specification
	Operating Current 70mA

	Source Specification
	Supported Card MIFARE One IC card

	Source Specification
	Operating Frequency IC (13.56MHz)

	Operating Environment Operating Temperature
	-10~50℃ Operating Humidity: <90%

	Source Specification
	Transmission Distance 80m max.

	Source Specification
	Reading Distance IC 3-5cm depending on card

	Source Specification
	Output Mode WG26/34or custom protocol






