FusWorth
DS-52
Product Specifications
	Specification
	Details

	Operating System
	Linux

	Liveness Detection
	Dual-camera liveness detection

	Camera
	MIPI+MIPI 2 MP

	Display
	5-inch HD display

	Touchscreen
	Capacitive touchscreen

	Supported Languages
	Chinese, English, Persian, Russian,Italian,Indonesian,Spanish,Vietnamese, Portuguese, Arabic, Thai,etc

	Power Supply
	DC12V/2A

	Operating Temperature & Humidity
	-30℃~60℃; 10~90%RH

	External Interfaces
	Wiegand Output (26/34), Relay Output, Exit Button, Doorbell

	Face Capacity
	1000

	Card Capacity
	1000

	Password Capacity
	1000

	Record Capacity
	100000

	Recognition Speed
	<0.5s

	Verification Methods
	Face/Card/Password/QR Code

	Card Reading
	Standard IC card reader

	Communication
	USB Flash Drive

	Dimensions
	192mm*86mm*22mm

	Protection Rating
	IP65 Waterproof and Dustproof

	Housing Material
	Flame-retardant ABS plastic






