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Product Specifications
	Specification
	Details

	Main Unit Dimensions (L*W*H)
	88*88*18.5mm

	Back Cover Dimensions (L*W*H)
	86*86*2mm

	Material
	Zinc alloy housing with acrylic panel

	Reader Interface
	WG26/34

	Decoding Support
	QR code

	Operating Voltage
	Supports 10–15 V input

	Operating Current
	220mA

	Image Sensor
	0.3 MP CMOS sensor (640*480 pixels) (640*480pixels)

	Scan Angle
	Tilt+-55°, Rotation360°

	Reading Distance
	from window surface5-20cm

	Scanning Features
	Auto sensing with buzzer indication

	Light Source
	Built-in LED light source; resistant to strong ambient light

	Decoding Mode
	Image decoding

	Operating Environment
	Temperature Range-25℃-55℃, Relative Humidity5%-95% (non-condensing)

	Card Reading
	Built-in IC card reader

	Reading Distance
	from window3-5cm

	Card Type
	Contactless IC card






