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Product Specifications
	Specification
	Details

	Source Specification
	Operating Voltage 12V~24Vwide-voltage design

	Source Specification
	Operating Current 500mA

	Source Specification
	Supported Readers 2

	Reader Protocol Network mode
	standard Wiegand 26/34; offline mode: dedicated protocol reader

	Source Specification
	Communication TCP/IP networking or offline card encoding

	User Capacity Networked
	10,000 (expandable); offline: unlimited

	Record Capacity Networked
	50,000 (expandable); offline: no record storage

	Source Specification
	Fire Alarm Linkage Interface 1

	Source Specification
	Manual Control Interface 1

	Source Specification
	Temperature & Humidity -10℃~60℃ (10~90%RHnon-condensing)

	Source Specification
	Secondary Development Supported (HTTP protocol)

	Source Specification
	Managed Floors Main board directly controls up to 16 floors

	Source Specification
	Expansion Board 16 floors each; up to 3 expansion boards can be added for direct control of 64 floors

	Source Specification
	Dimensions 180mm*120mm*15mm






