FusWorth
J-55A
Product Specifications
Basic Information
	Specification
	Details

	Device Category
	Facial Recognition Terminal

	Screen
	5-inch IPS high-definition display

	Protection Rating
	IP65


Capacity
	Specification
	Details

	Face Capacity
	20,000

	Card Capacity
	20,000

	Password Capacity
	10,000

	Fingerprint Capacity
	10,000

	Palmprint Capacity
	1,000

	Record Capacity
	200,000


Identification
	Specification
	Details

	Verification Methods
	Face / IC card / Password / Fingerprint / Palmprint


Communication and Access
	Specification
	Details

	Communication Method
	TCP/IP, USB (optional WiFi/4G)


Physical Specifications
	Specification
	Details

	Dimensions
	204 × 90 × 23 mm






