FusWorth
JF-52A
Product Specifications
	Specification
	Details

	Operating System
	Linux

	Liveness Detection
	Dual-camera liveness detection

	Camera
	: RGB+IR 2 MP

	Display
	5-inch HD display

	Touchscreen
	Capacitive touchscreen

	Supported Languages
	Chinese, English, Persian, Russian,Italian,Indonesian,Spanish,Vietnamese, Portuguese, Arabic, Thai,etc

	Power Supply
	DC12V/2A

	Operating Temperature & Humidity
	-30℃~60℃; 10~90%RH

	External Interfaces
	Wiegand Output (26/34), Relay Output, Ethernet Port, Exit Button, Doorbell

	Face Capacity
	2000

	Card Capacity
	2000

	Password Capacity
	2000

	Fingerprint Capacity
	4000

	Palm Vein Capacity
	500

	Record Capacity
	100,000

	Recognition Speed
	<0.5s

	Verification Methods
	Face/Card/Password/Fingerprint/Palm Vein/QR Code

	Card Reading
	Standard IC card reader

	Communication
	USB Flash Drive/TCP/IP (Optional WiFi/4G)

	Dimensions
	192mm*86mm*22mm

	Protection Rating
	IP65 Waterproof and Dustproof

	Housing Material
	Flame-retardant ABS plastic






