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JF-52AT
Product Specifications
	Specification
	Details

	Operating System
	Linux

	Power Supply
	DC12V/2A

	Operating Temperature & Humidity
	-40℃~70℃; 10~90%RH

	Display
	5-inch IPS HD display

	Face Capacity
	2000

	Card Capacity
	2000

	Password Capacity
	2000

	Fingerprint Capacity
	4000

	Palm Capacity
	500

	Record Capacity
	100000

	Recognition Speed
	<0.5s

	Supported Languages
	Chinese, English

	Controllable Floors
	Standard face terminal + 16-floor expansion board; supports up to 4 expansion boards, controlling up to 64 floors

	Verification Methods
	Face/Card/Fingerprint/Palm/Password/QR Code

	Waterproof
	IP65

	Communication
	USB Flash Drive/TCP/IP (Optional WiFi/4G)

	Dimensions
	192mm*86mm*22m






