FusWorth
LX01
Product Specifications
	Specification
	Details

	Dimensions
	106mm*82mm*25mm

	Reading Distance
	＞70mm

	Reading Time
	＜100ms

	Input Format
	MIFARE One IC card

	Output
	Wiegand output, high-speed USB interface

	Power Supply
	USB powered

	Source Specification
	Operating Temperature -10℃～50℃

	Source Specification
	Operating Humidity 5%～95%






