FusWorth
S20-KE
Product Specifications
	Specification
	Details

	Source Specification
	Offline sector encoding, waterproof, with keypad

	Input Voltage
	DC12V (+-10%)

	Card Type
	M1 cardIC

	Reading Distance
	5-8CM (depending on card)

	Controlled Doors
	1

	Dimensions
	107*74*19mm

	Authorization Method
	Offline Card Encoding

	Card Capacity
	Unlimited (offline card encoding)

	Software Version
	Mjsystem 3.0






