FusWorth
S25-C
Product Specifications
	Specification
	Details

	Source Specification
	IC master card authorization, waterproof

	Dimensions
	88*88*18mm

	Input Voltage
	DC12V (+-10%)

	Operating Current
	Standby Current≤100mA, Active Current≤200mA

	Card Type
	M1 cardIC

	Reading Distance
	5-8CM (depending on card)

	Controlled Doors
	1

	Authorization Method
	Master card

	Card Capacity
	Master card: 10,000

	Source Specification
	Supports WG26/WG34 input for external readers






