FusWorth
S25-D
Product Specifications
	Specification
	Details

	Source Specification
	ID master card, waterproof

	Dimensions
	88*88*18mm Input Voltage: DC12V (+-10%) Operating Current: Standby Current≤100mA, Active Current≤200mA

	Card Type
	EM cardID

	Reading Distance
	5-8CM (depending on card)

	Controlled Doors
	1

	Authorization Method
	Master card

	Card Capacity
	Master card: 10,000 Supports WG26/WG34 input for external readers






