FusWorth
S25-KEF
Product Specifications
	Specification
	Details

	Source Specification
	Offline card encoding, anti-copy, waterproof, with keypad

	Dimensions
	86*86*18mm

	Operating Voltage
	12VDC; Standby Current≤100mA, Active Current≤200mA

	Authorization Method
	Offline Card Encoding

	Card Type
	M1 cardIC

	Recognition Distance
	3-8cm (depending on card)

	Protection Rating
	IP65 (Waterproof and Dustproof)

	Operating Conditions
	Temperature: -10℃-45℃;Relative Humidity: 20%-90%






