FusWorth
T5
Product Specifications
	Specification
	Details

	Source Specification
	Dedicated offline card reader

	Dimensions
	62.5*42.5*5mm

	Source Specification
	Standard Complies with ISO/IEC 14443 Type A

	Source Specification
	Housing Material Plastic

	Source Specification
	Operating Voltage 9-12VDC

	Source Specification
	Operating Current 70mA

	Source Specification
	Supported Card MIFARE One IC card

	Source Specification
	Keypad None

	Source Specification
	Operating Frequency IC (13.56MHz)

	Operating Environment Operating Temperature
	-10~50℃ Operating Humidity: <90%

	Source Specification
	Reading Distance IC 3-5cm depending on card

	Source Specification
	Output Mode WG26/34or custom protocol

	Source Specification
	Pulse Output Negative pulse widthTP=100μs, Pulse periodTW=2ms






