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Product Specifications
	Specification
	Details

	Source Specification
	2-Door Two-Way Control Board

	Dimensions
	160*129mm

	Communication
	TCP/IP

	Record Capacity
	50000

	Card Capacity
	30000

	Password Capacity
	2 super passwords

	Source Specification
	Personal password count corresponds to card count

	Controlled Doors
	2

	External Card Readers
	Supports 4 external readers

	External Switches
	2

	Supported Reader Protocol
	WG26/34

	Software
	B/S Management Platform

	SupportedDatabase
	SQL






