FusWorth
DF-10
Product Specifications
	Specification
	Details

	Source Specification
	1-Door Two-Way Controller

	Dimensions
	160*129mm

	Communication
	TCP/IP

	Record Capacity
	50000

	Card Capacity
	30000

	Password Capacity
	2 super passwords

	Source Specification
	Personal password count corresponds to card count

	Controlled Doors
	1

	External Card Readers
	Supports 2 external readers

	External Switches
	1

	Supported Reader Protocol
	WG26/34

	Software
	V6.0

	SupportedDatabase
	Access, SQL






