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F30
Product Specifications
	Specification
	Details

	Source Specification
	Basic Fingerprint Standalone Terminal

	Dimensions
	86*86*26mm

	Display
	Monochrome display

	Fingerprint Recognition Time
	<1.5S

	False Rejection Rate
	< 0.01%

	False Acceptance Rate
	< 0.0001%

	Fingerprint Capacity
	500

	Proximity Card Capacity
	500

	Password Capacity
	2

	Controlled Doors
	1

	Authentication Methods
	Fingerprint, Password, ID/IC card (Card reading is not standard and requires customization)






