FusWorth
J-54
Product Specifications
Basic Information
	Specification
	Details

	Device Category
	Facial Recognition Terminal

	Screen
	5-inch IPS high-definition display

	Protection Rating
	IP65


Capacity
	Specification
	Details

	Face Capacity
	5,000

	Card Capacity
	10,000

	Password Capacity
	10,000

	Palmprint Capacity
	1,000

	Record Capacity
	200,000


Identification
	Specification
	Details

	Verification Methods
	Face / IC card / Password / Palmprint


Communication and Access
	Specification
	Details

	Communication Method
	TCP/IP, USB (optional WiFi/4G)


Physical Specifications
	Specification
	Details

	Dimensions
	198 × 86 × 17 mm






