FusWorth
L60-EF
Product Specifications
	Specification
	Details

	Source Specification
	Anti-copy

	Input Voltage
	DC12V (+-10%)

	Card Type
	M1 card

	Reading Distance
	3-5CM (depending on card)

	Controlled Doors
	1

	Dimensions
	68.8*45.9mm

	Software Version
	Building Access Control Management Software3.0

	Card Capacity
	Unlimited

	Anti-copyFunction
	Optional

	Data Capacity
	None

	Registration Method
	Offline Card Encoding






