FusWorth
S20-D
Product Specifications
	Specification
	Details

	Source Specification
	ID master card authorization, waterproof

	Input Voltage
	DC12V (+-10%)

	Card Type
	EM cardID

	Reading Distance
	5-8CM (depending on card)

	Controlled Doors
	1

	Dimensions
	107*74*19mm

	Authorization Method
	Master card

	Card Capacity
	Master card: 10,000

	Source Specification
	Supports WG26/WG34 input for external readers






