FusWorth
S25-KD
Product Specifications
	Specification
	Details

	Source Specification
	ID master card / keypad authorization, waterproof

	Dimensions
	88*88*18mm

	Input Voltage
	DC12V (+-10%)

	Operating Current
	Standby Current≤100mA, Active Current≤200mA

	Card Type
	EM cardID

	Reading Distance
	5-8CM (depending on card)

	Controlled Doors
	1

	Authorization Method
	Master card, keypad

	Card Capacity
	Master card: 10,000, keypad: 1,000

	Source Specification
	Supports WG26/WG34 input for external readers






