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Product Specifications
	Specification
	Details

	Source Specification
	Dimensions 167.5*79.8*25mm

	Source Specification
	Display 2.4-inchcolor display

	Source Specification
	Keys 16 touch keys

	Source Specification
	Display Language Simplified Chinese

	Source Specification
	Power 12VDC, 100mA

	Source Specification
	Operating Mode Networked / Offline

	Source Specification
	Communication TCP/IP

	Source Specification
	Authentication Methods Fingerprint, IC card, Password

	Source Specification
	Combination Modes Fingerprint/Card/Password, Card+Password,Fingerprint+Card, Fingerprint+Password, Fingerprint, Card

	Source Specification
	Operating Humidity 20%~60%

	Source Specification
	Operating Temperature -30℃~45℃

	Source Specification
	Fingerprint Capacity 3,000 fingerprints

	Source Specification
	Password Capacity 3,000 personal passwords, 2 super passwords

	Source Specification
	Proximity Cards 3000

	Source Specification
	Record Capacity 50,000

	Source Specification
	Waterproof Yes

	Source Specification
	Time Group Management Supported

	Source Specification
	USB Flash Drive Supported

	Source Specification
	External Interfaces Wiegand Input/Output, Relay Output*1, Ethernet Port*1, Exit Button*1, Doorbell*1, Door Sensor*1, Fire Alarm*1






